Installation and customize:
Double click the setup file,SK6281_Win98Drv_yyyymmdd.exe. The default vid is 
1516 and pid is 8628 or 1603. If attemping to use the USB flash drive with different vid
and pid, just modify vidpid.txt before double clicking the setup file. 
The two files, pidvid.txt and SK6281_Win98Drv_yyyymmdd.exe, MUST be in the same directory.

Notes:
USB host controller driver MUST be installed properly first. If NOT, OS may not 
detect the USB flash drive or the USB flash drive can not work.
